Commodity Description

관세분류번호 HSK NO.	품목번호 Item NO	품명 및 규격서 Description	단위 Unit	수량 Q'ty
8442-30-2000	1	10,000kN Hydraulic Servo press (서보제어 프레스)	set	1

1. End-user’s Use

A. This machine is an 2-axis hydraulic forging press with servo valves control a main press of 10000kN(minimum),  and a bed knockout of 2000kN(minimum).

B. The main unit frame has a strong steel plate welded integral structure and is worked by high precision processing on the well annealed high rigidity materials. The parallelism of the slide is maintained by an eight-way guide.

C. Two operations mode of inching and one-stroke using a push-button are available. Positions, pressure and speed of all axis are adjustable. In addition, block forming and back pressure forming are possible for a severe tests of the various environments.

D. Motion data input should be possible in a table format using a computer, a motion process and timing for each axis can be created and registered as user wish. The actual motion diagram can be output during forming so that you can easily extract the forging data to adjust a forming condition.

2. Component

A. Press body

B. Hydraulic unit

C. Control board

D. Operation panel

E. Two-hand operation stand

F. Emergency stop push button

G. Automatic centralized lubrication (grease)

H. Light curtain (front)

I. Hydraulic die lifter

J. Die clamper

K. Pre-roller

L. Actual measurement editing software or similar function program

M. Handrail of deck

3. SPECIFICATION

A. Main

A-1. Capacity : 10000kN or more .

A-2. Stroke : 500mm or more.

A-3. Descending and rising speed : 200mm/s

A-4. Pressing speed : 0.1 ~4mm/s or more. (depending on the pressure)

A-5. Upper and lower bolster area : 1000mm by 1000mm or more

A-6. Repeatability of positioning precision : ± 0.05mm or less

A-7. Repeatability of loading precision : ± 5% or less (all working position)

B. Bottom Knockout

B-1. Capacity : 2000kN or more.

B-2. Stroke : 200mm or more.

B-3. Speed : 5mm/s or less

B-4. Control method : servo valve control

C. Operating supplies

C-1. Real-time motion control and data acquisition system(data log)

C-2. Safety devices(emergency stop function and etc...)

C-3. Die lifter(pre-roller), die clamper and etc...

D. Operation

D-1. Tool change operation

D-2. Manual operation(each axis can be operated by manual respectively)

D-3. Continuous operation

4. SPECIAL NOTE

A. The seller of the equipment is fully responsible for training the user about operating and maintaining the equipment free of charge.

B. The equipment is to be warranted for 1 year after purchase(successful installation) or 2000 hours after purchase(successful installation), it and for making it ready to use at the time of equipment arrival.